**F registers on the locomotives**

This is the byte following the address byte(s)

F4 – F1 100xxxxx

 04321

 0 Light

 1 Sound

 2 Horn 1

 3 Horn 2

 4 Bell

F8 – F5 1011xxxx

 8765

F12 – F9 1010xxxx

 111

 2109

F20 – F13 1101xxxx

Bit values: 1 = on 0 = off