**F registers on the locomotives**

This is the byte following the address byte(s)

F4 – F1 100xxxxx

04321

0 Light

1 Sound

2 Horn 1

3 Horn 2

4 Bell

F8 – F5 1011xxxx

8765

F12 – F9 1010xxxx

111

2109

F20 – F13 1101xxxx

Bit values: 1 = on 0 = off